Markgröningen, 24.11.2017

Suspended in no time - with the new crane hooks from norelem

A comprehensive range of crane hooks for various lifting applications

**The norelem crane hooks are connecting elements between the hoist and the lifting chain or textile sling. They can be used for lifting weights of up to 10 tonnes and are produced to meet the current safety requirements.**

At norelem designers can find all conventional hook types with eye or clevis. The latter are supplied with bolt and pin and enable direct mounting on the chain without the need of intermediate links. These crane hooks are suitable for chains of nominal size 6 to 16 mm and, as previously mentioned can be used to lift weights of up to 10 tonnes. All models have a high quality safety catch which prevents the load slipping off. The self-locking hooks 07792 and the swivel hooks 07794 close and lock automatically under load and so, offer the user even more safety.

The round sling hooks 07796 are best suited for quick lifting jobs using lifting tackle such as flat or round textile slings. These also have a robust, forged safety catch. All edges are rounded to protect the textile lifting tackle. The colour of the round sling hooks corresponds to the colour code assigned to textile lifting tackle that signifies the permissible loads.

All crane hooks in the norelem range are manufactured according the current safety regulations and correspond to the Machinery Directive and are BG certified (H stamp). The crane hooks from norelem are available as high quality grade 10, the round sling hooks and matching links are grade 8.

Characters including spaces: 1,579

Brief profile of norelem Normelemente KG

Every success begins with an idea. This is why norelem supports you in achieving your targets in machine and plant construction with an unrivalled selection of standard parts and components. THE BIG GREEN BOOK offers designers and technicians an extensive and clearly arranged assortment of quality components.

We support your project right from the start - with expert advice, a complete CAD database and fast delivery. norelem has been dynamically evolving for almost 60 years, consistently amending our portfolio and continuously optimising the logistics.

From our headquarters in Markgröningen, Germany and over our international locations, we are active in youth developement with schooling and workshops.

Characters including spaces: 709