Markgröningen, 13.08.2019

**Pin and clevis heads in the new versions**

A total of five new models have now been added to the full norelem range

**With norelem, engineers have an even greater selection available in the pin and clevis area. These components can be used to create fully functional clevis joints.**

Three new clevis head pins are now available from norelem. These include [a model](https://www.norelem.co.uk/gb/en/Products/Product-overview/Systems-and-components-for-machine-and-plant-construction/27000-Clevis-joints-Rod-ends-Ball-joints-Axial-joints-Levelling-sets-Swivel-feet-Levelling-feet-Tube-end-plugs-Equipment-feet-Hinges/Rod-ends/27621-01-Pin-with-circlip-groove-suitable-for-clevis-joints.html?search_keywords=27621-01) 27621-01 with a groove for securing shafts using a lock washer for DIN 6799 shafts. Alternatively, users can apply a KL or SL retainer.

[Another pin](https://www.norelem.co.uk/gb/en/Products/Product-overview/Systems-and-components-for-machine-and-plant-construction/27000-Clevis-joints-Rod-ends-Ball-joints-Axial-joints-Levelling-sets-Swivel-feet-Levelling-feet-Tube-end-plugs-Equipment-feet-Hinges/Rod-ends/27621-02-Pin-with-circlip-groove-suitable-for-clevis-joints.html?search_keywords=27621-02) is also available 27621-02 with a groove for inserting a DIN 471 circlip. On the other hand, the third [new pin](https://www.norelem.co.uk/gb/en/Products/Product-overview/Systems-and-components-for-machine-and-plant-construction/27000-Clevis-joints-Rod-ends-Ball-joints-Axial-joints-Levelling-sets-Swivel-feet-Levelling-feet-Tube-end-plugs-Equipment-feet-Hinges/Rod-ends/27621-03-Pin-with-hole-for-split-pin-suitable-for-clevis-joints.html?search_keywords=27621-03) 27621-03 uses a cotter.

In the clevis head area, norelem is offering [new models](https://www.norelem.co.uk/gb/en/Products/Product-overview/Systems-and-components-for-machine-and-plant-construction/27000-Clevis-joints-Rod-ends-Ball-joints-Axial-joints-Levelling-sets-Swivel-feet-Levelling-feet-Tube-end-plugs-Equipment-feet-Hinges/Clevis-joints/27624-05-Clevis-steel-or-stainless-steel-with-male-thread.html?search_keywords=27624-05) with item number 27624-05 which are made of steel or stainless steel with external thread. [Suitable steel counterpieces](https://www.norelem.co.uk/gb/en/Products/Product-overview/Systems-and-components-for-machine-and-plant-construction/27000-Clevis-joints-Rod-ends-Ball-joints-Axial-joints-Levelling-sets-Swivel-feet-Levelling-feet-Tube-end-plugs-Equipment-feet-Hinges/Clevis-joints/27624-10-Clevis-tang-steel.html?search_keywords=27624-10+) are also available: these can be combined with DIN 71752 clevis heads and clevis joints. These products are used for connections which have to compensate for a direction offset in one direction.

Characters including spaces: 1,008

Brief profile of norelem Normelemente KG

Every success begins with an idea. This is why norelem supports you in achieving your targets in machine and plant construction with an unrivalled selection of standard parts and components. THE BIG GREEN BOOK offers designers and technicians an extensive and clearly arranged assortment of quality components.

We support your project right from the start - with expert advice, a complete CAD database, and fast delivery. For over 60 years norelem has been dynamically evolving, consistently amending our portfolio and continuously optimising the logistics.

From our headquarters in Markgröningen, Germany and over our international locations, we are active in youth developement with schooling and workshops.

Characters including spaces: 707